<http://hazard.com/msds/f2/bwb/bwbhl.html>

AERVOE-PACIFIC CO INC -- 16A PRIMERS, 127 BLACK -- 8010-00N055488 ===================== Product Identification =====================

Product ID:16A PRIMERS, 127 BLACK

MSDS Date:01/19/1993

FSC:8010

NIIN:00N055488

MSDS Number: BWBHL

=== Responsible Party ===

Company Name:AERVOE-PACIFIC CO INC

Address:1198 SAWMILL RD

City:GARDNERVILLE

State:NV

ZIP:89410

Country:US

Emergency Phone Num:800-424-9300 (CHEMTREC)

CAGE:0UPL1

=== Contractor Identification ===

Company Name:AERVOE-PACIFIC CO INC

Address:1198 SAWMILL RD

Box:City:GARDNERVILLE

State:NV

ZIP:89410

Country:US

Phone:702-782-0100

CAGE:0UPL1

============= Composition/Information on Ingredients =============

Ingred Name:XYLENE (SARA III). LD50:(ORAL,RAT)4300MG/KG

CAS:1330-20-7

RTECS #:ZE2100000

Fraction by Wt: 14%

OSHA PEL:100 PPM

ACGIH TLV:100 PPM/150 STEL

EPA Rpt Qty:1000 LBS

DOT Rpt Qty:1000 LBS

Ingred Name:ACETONE (SARA III). LD50:(ORAL,RAT)9750MG/KG

CAS:67-64-1

RTECS #:AL3150000

Fraction by Wt: 14%

OSHA PEL:1000 PPM

ACGIH TLV:750PPM/1000 STEL

EPA Rpt Qty:5000 LBS

DOT Rpt Qty:5000 LBS

Ingred Name:PROPANE

CAS:74-98-6

RTECS #:TX2275000

Fraction by Wt: 15%

OSHA PEL:1000 PPM

ACGIH TLV:ASPHYXIANT

Ingred Name:PROPANE, 2-METHYL-; (ISOBUTANE)

CAS:75-28-5

RTECS #:TZ4300000

Fraction by Wt: <5.0%

OSHA PEL:800 PPM (MFR)

ACGIH TLV:800 PPM (MFR)

Ingred Name:BUTANE

CAS:106-97-8

RTECS #:EJ4200000

Fraction by Wt: 5%

OSHA PEL:800 PPM

ACGIH TLV:800 PPM

Ingred Name:VOLATILE ORGANIC CONTENT:5.31 LBS/IMP GAL 4.42LBS/US GAL

530GMS/LTR

RTECS #:9999999VO

OSHA PEL:N/K

ACGIH TLV:N/K

===================== Hazards Identification =====================

LD50 LC50 Mixture:SEE INGREDIENTS

Routes of Entry: Inhalation:YES Skin:YES Ingestion:YES

Reports of Carcinogenicity:NTP:NO IARC:NO OSHA:NO

Health Hazards Acute and Chronic:ACUTE:INHALATION:ANESTHETIC.

IRRITATION OF THE RESPIRATORY TRACT, OR NERVOUS SYSTEM

DEPRESSION-CHARACTERIZED BY HEADACHE, DIZZINESS, NAUSEA, OR

POSSIBLE UNCONSCIOUSNESS. SKIN OR EYE CONT:PRIMARY IRRIT ATION.

PROLONGED OR REPEATED CONT TO SKIN MAY CAUSE DERMATITUS - EXERCISE

DUE CARE.

Explanation of Carcinogenicity:NOT RELEVANT.

Effects of Overexposure:SEE HEALTH HAZARDS.

Medical Cond Aggravated by Exposure:NONE KNOWN.

======================= First Aid Measures =======================

First Aid:INGEST:CALL MD IMMEDIATELY . INHAL:REMOVE FROM EXPOSURE AND

RESTORE BREATHING, SEEK MEDICAL ATTN. SKIN:WASH AFFECTED AREA,

REMOVE CONTAMD CLTHG, SEE PHYS IF ANY IRRITATION PERSISTS.

EYES:FLUSH I MMEDIATELY WITH WATER FOR @ LEAST 15 MINUTES - TAKE TO

PHYSICIAN.

===================== Fire Fighting Measures =====================

Flash Point Method:TCC

Flash Point:-22F,-30C

Lower Limits:1.0%

Upper Limits:12.8%

Extinguishing Media:FOAM, ALCOHOL FOAM, CO\*2, DRY CHEMICAL, WATER FOG.

Fire Fighting Procedures:NIOSH/MSHA APPRVD SCBA & FULL PROT EQUIP .

WATER SPRAY MAY BE INEFTIVE, BUT WATER SPRAY MAY BE USED TO COOL

CNTNRS EXPOS TO HEAT/FIRE TO (SUPDAT)

Unusual Fire/Explosion Hazard:CLOSED CONTAINERS MAY EXPLODE DUE TO

BUILD UP OF PRESSURE FROM EXTREME HEAT OR FIRE. AEROSOL SPRAY IS

EXTREMELY FLAMMABLE.

================== Accidental Release Measures ==================

Spill Release Procedures:REMOVE ALL SOURCES OF IGNITION; FLAMES,

SPARKS, STATIC ELECTRICITY & ELECTRICAL. VENTILATE AREA & SOAK UP

WITH INERT ABSORBENT USING NON-SPARKING TYPE TOOLS.

Neutralizing Agent:NONE SPECIFIED BY MANUFACTURER.

====================== Handling and Storage ======================

Handling and Storage Precautions:DO NOT STORE ABOVE 120F. DO NOT

STORE/USE NEAR HEAT, SPARKS, OR FLAME. DO NOT GET IN EYES. DO NOT

BREATHE VAP. AVOID SKIN CONT.

Other Precautions:DO NOT TAKE INTERNALLY. SMOKING WHILE USING THIS PROD

MUST BE STRICTLY PROHIBITED. IN ADDTN TO ALL OTHER HAZARDS &

PRECAUT - DUST FROM SANDING THE DRY PAINT FILMS SHOULD BE TREATED

AS NUISANCE DUST W/ TLV OF 10 MG/CUBIC METER.

============= Exposure Controls/Personal Protection =============

Respiratory Protection:OUTDOORS:WE REC AN NIOSH/MSHA APPRVD PARTICULATE

FILTER TO REMOVE ANY AIRBORNE OVERSPRAY. IN RESTRICTED AREAS W/POOR

VENT & CLOSE TO TLV, NIOSH/MSHA APPRVD RESP W/ORGANIC VAPOR

CARTRIDGE IS RECOMMENDE D.

Ventilation:ALL APPLIC AREAS SHOULD BE ADEQUATELY VENTILATED IN ORDER

TO KEEP THE INGEDS BELOW THEIR EXPOSURE LIMITS.

Protective Gloves:IMPERVIOUS GLOVES.

Eye Protection:SFTY GLASSES W/SIDE SHIELDS.

Other Protective Equipment:EYE WASH FOUNTAIN & SAFETY SHOWER.

IMPERVIOUS APRON IS RECOMMENDED TO PREVENT SKIN CONTACT.

Work Hygienic Practices:AVOID PROLONGED OR REPEATED CONT. DO NOT

BREATHE VAPORS. WASH CONTAMINATED CLOTHING PRIOR TO RE-USE.

Supplemental Safety and Health

FIRE FIGHT PROC:PREVENT PRESSURE BUILD UP.

================== Physical/Chemical Properties ==================

HCC:V3

Boiling Pt:B.P. Text:-10F,-23C

Vapor Density:HVR/AIR

Spec Gravity:0.9 (H\*20=1)

Evaporation Rate & Reference:FASTER/N-BUTYL ACETATE

Solubility in Water:NEGLIGIBLE

Appearance and Odor:OPAQUE LIQUID/SOLVENT BASED ODOR

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

STRONG OXIDIZING AGENTS.

Stability Condition to Avoid:HIGH TEMPERATURES.

Hazardous Decomposition Products:CARBON MONOXIDE, CARBON DIOXIDE AND

VARIOUS HYDROCARBONS.

==================== Disposal Considerations ====================

Waste Disposal Methods:DISPOSE OF IN ACCORDANCE WITH LOCAL, STATE, AND

FEDERAL REGULATIONS. DO NOT INCINERATE CLOSED CONTAINERS.

Disclaimer (provided with this information by the compiling agencies):

This information is formulated for use by elements of the Department

of Defense. The United States of America in no manner whatsoever,

expressly or implied, warrants this information to be accurate and

disclaims all liability for its use. Any person utilizing this

document should seek competent professional advice to verify and

assume responsibility for the suitability of this information to their

particular situation.